crs_wkt {INLA} | R Documentation

## Handling CRS/WKT

### Description

in favour of `fmesher::fm_wkt()` and related methods.

Get and set CRS object or WKT string properties.

### Usage

    inla.wkt_is_geocent(wkt)

    inla.crs_is_geocent(crs)

    inla.wkt_get_ellipsoid_radius(wkt)

    inla.crs_get_ellipsoid_radius(crs)

    inla.wkt_set_ellipsoid_radius(wkt, radius)

    inla.crs_set_ellipsoid_radius(crs, radius)

    inla.wkt_unit_params()

    inla.wkt_get_lengthunit(wkt)

    inla.wkt_set_lengthunit(wkt, unit, params = NULL)

    inla.crs_get_wkt(crs)

    inla.crs_get_lengthunit(crs)

    inla.crs_set_lengthunit(crs, unit, params = NULL)

### Arguments

`wkt` | A WKT2 character string
`crs` | A `sp::CRS` or `inla.CRS` object
`radius` | numeric
`unit` | character, name of a unit. Supported names are "metre", "kilometre", and the aliases "meter", "m", International metre", "kilometer", and "km", as defined by `inla.wkt_unit_params` or the `params` argument. (For legacy PROJ4 use, only "m" and "km" are supported)
`params` | Length unit definitions, in the list format produced by `inla.wkt_unit_params()`, Default: NULL, which invokes `inla.wkt_unit_params()`

### Value

For `inla.wkt_unit_params`, a list of named unit definitions

For `inla.wkt_get_lengthunit`, a list of length units used in the wkt string, excluding the ellipsoid radius unit.

For `inla.wkt_set_lengthunit`, a WKT2 string with altered length units. Note that the length unit for the ellipsoid radius is unchanged.

For `inla.crs_get_wkt`, WKT2 string.

For `inla.crs_get_lengthunit`, a list of length units used in the wkt string, excluding the ellipsoid radius unit. (For legacy PROJ4 code, the raw units from the proj4string are returned, if present.)

For `inla.crs_set_lengthunit`, a `sp::CRS` object with altered length units. Note that the length unit for the ellipsoid radius is unchanged.

For `inla.wkt_unit_params`, a list of named unit definitions

For `inla.wkt_get_lengthunit`, a list of length units used in the wkt string, excluding the ellipsoid radius unit.

For `inla.wkt_set_lengthunit`, a WKT2 string with altered length units. Note that the length unit for the ellipsoid radius is unchanged.

For `inla.crs_get_wkt`, WKT2 string.

For `inla.crs_get_lengthunit`, a list of length units used in the wkt string, excluding the ellipsoid radius unit. (For legacy PROJ4 code, the raw units from the proj4string are returned, if present.)

For `inla.crs_set_lengthunit`, a `sp::CRS` object with altered length units. Note that the length unit for the ellipsoid radius is unchanged.

### Functions

- `inla.wkt_is_geocent()`: in favour of `fmesher::fm_wkt_is_geocent()`

- `inla.crs_is_geocent()`: in favour of `fmesher::fm_crs_is_geocent()`

- `inla.wkt_get_ellipsoid_radius()`: in favour of `fmesher::fm_ellipsoid_radius()`

- `inla.crs_get_ellipsoid_radius()`: in favour of `fmesher::fm_ellipsoid_radius()`

- `inla.wkt_set_ellipsoid_radius()`: in favour of `fmesher::fm_wkt_set_ellipsoid_radius()`

- `inla.crs_set_ellipsoid_radius()`: in favour of `fmesher::fm_ellipsoid_radius<-()`

### Author(s)

Finn Lindgren finn.lindgren@gmail.com

### See Also

`inla.sp_get_crs()`

`inla.sp_get_crs()`

### Examples

    ## Not run:
    c1 <- fmesher::fm_crs("globe")
    inla.crs_get_lengthunit(c1)
    c2 <- inla.crs_set_lengthunit(c1, "metre")
    inla.crs_get_lengthunit(c2)

    ## End(Not run)

    ## Not run:
    c1 <- inla.CRS("globe")
    inla.crs_get_lengthunit(c1)
    c2 <- inla.crs_set_lengthunit(c1, "km")
    inla.crs_get_lengthunit(c2)

    ## End(Not run)

[Package INLA version 26.02.05 Index]